**Questionnaire for FIBCs / Big Bags / Jumbo Bags**

|  |  |  |  |
| --- | --- | --- | --- |
| Customer: |  | Date: |  |
| Contact tel: |  | E-mail: |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Type** | | **Design Variants** | | | | | | | | | | | | | | | |
| Top  Type | | 1 | | Открытый верх | | 2 | | Насыпный клапан | | | 3 | Фартук | | | 4 | Лацкан | |
|  | |  | |  |  |
| Open | | | | Filling spout | | | | | Skirt | | | | Flap | | |
| I | С одной рукой подъема | Биг%20бег | | | | | | | | | | | | | | | |
| II | С двумя  руками подъема |
| III | Классический |
| Type  Bottom | | 1 | Плоское дно | | 2 | | C:\Users\dyshl\Desktop\картинки\43Безымянный.jpg | | 3 | Высыпный клапан | | | 4 | C:\Users\dyshl\AppData\Local\Microsoft\Windows\INetCache\Content.Word\Бе5432542зымянный.jpg | | 5 | Фартук с парусинками |
|  |  | |  |  |  |
| Flat | | | Star-shaped | | | | Discharge spout | | | | Spout with safety valve | | | Emptying skirt with flap | |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Technical data** | **Indicator values** | | | | | | |
| \*Filling product |  | | | | | |  |
| \*Filling product weight |  | | | | | | [kg] |
| \*Filling product bulk weight |  | | | | | | [kg/m³] |
| \*Design | Type |  | Top |  | Bottom |  |  |
| \*Sizes | A |  | B |  | C |  | [cm] |
| D |  | E |  | Ft |  | [cm] |
| Ht |  | Fb |  | Hb |  | [cm] |
| \*Printing |  | | | | | | [yes / no] |
| Printing colors quantity |  | | | | | | [1-6] |
| \*Charging level |  | | | | | | [cm] |
| \*Operating loop length |  | | | | | | [cm] |
| \*Innerliner |  | | | | | | [yes / no] |
| Innerliner thickness |  | | | | | | [um] |
| Innerliner width |  | | | | | | [cm] |
| Innerliner length |  | | | | | | [cm] |
| Bag weight |  | | | | | | [g] |
| \*Total bag weight |  | | | | | | [g/m²] |
| \*Total bag quantity |  | | | | | | [pcs] |
| Additional data |  | | | | | |  |

\*For pricing you should fill in all the marked lines.